INTERFACE 800,230
VSTVARS 6
VSTVAR 0, .94, "LPROOMSIZE", "", .9, .9999, 0
VSTVAR 1, .92, "HPROOMSIZE", "", .9, .9999, 0
VSTVAR 2, 5000, "F Thres", "Hz", 10, 20000, 0
VSTVAR 3, 50, "Dry/Wet", "%", 0, 100, 1
VSTVAR 4, 0, "Pre-Delay", "ms", 0, 100, 1
VSTVAR 5, 1, "RVB Wide", "", 0, 5, 1

TOOLTIP "Reverb widening. ( 混响扩展 )\nSet this parameter to 0 to have a monophonic REVERB.\nIncrease to increase wideness.", 5
TOOLTIP "Pre-Delay control: the REVERB starts after this delay.", 4
TOOLTIP "Dry/Wet control.", 3
TOOLTIP "Frequency threshold between low and high portion of the spectrum.", 2
TOOLTIP "Feedback for the high portion of the spectrum ('Room size').", 1
TOOLTIP "Feedback for the low portion of the spectrum ('Room size').", 0

//UIMOD 709,0,0,0
//UIMOD 710,0,0,0
UIMOD 710,255,255,255
UIMOD 712,0,0,0
UIMOD 711,255,255,255 
//UIMOD 0,100,0,3,50,0,0,0,0,0,0,0,0,0
//UIMOD 0,100,0,3,50,90,90,90,70,70,70,70,70,120
//UIMOD 2,250,23,48,900,0,0,0
UIMOD 2,250,23,48,900,255,255,255
KNOB 0, "D100;Iknob_solid_alum.bmp;L6;T3"

POST
IF MCC(603)<.1 EXIT
OUT=.01*((100-MCC(603))*OUT+MCC(603)*WIDE(DELAY(REVERB(OUT,MCC(600),MCC(601),MCC(602),-1),MCC(604)*.001),MCC(605)))
